510   SEDAN               01All 510 sedans.
510   WAGON               01All 510 wagons.
510   3-SPEED             01510 model with a 3-speed manual transmission.
510   4-SPEED             01510 model with a 4-speed manual transmission.
510   AUTOMATIC(or AUTO)  01510 model with an automatic transmission.
510   L13                 01510 model with a 1,296cc(79.1 cu.in.)engine.
510   L16                 01510 model with a 1,595cc(97.3 cu.in.)engine.
510   CANADA              01510 model for CANADA from 1969 model with safety dev510   CANADA              02ices.
510   CRANK               01L16 engine with crankcase emission control devices .510   4-DOOR              01All 510 4-DOOR Sedan and Wagon.
510   2-DOOR              01ALL 510 2-DOOR Sdan.
510   EVAPO               01L16 engine with evaporative emission control devices510   EVAPO               01for California only.
510   EXHAUST             01L16 engine with exhaust emission control devices for510   EXHAUST             02Ontario and USA except California.
510   USA-S               01U.S.A. with both emission control devices and safty 510   USA-S               02devices.
510   USA                 01U.S.A. (including EVAPO.EXHAUST and USA-S)
510   AMERICA             01NORTH AMERICA and SOUTH AMERICA.
510   OP                  01Optional equipped.
510   ONLY                01ONLY is used together with the destination.
510   EXC                 01Except.
510   INC                 01Including.
